# *ANNEX II + III:* TECHNICAL SPECIFICATIONS + TECHNICAL OFFER

**Contract title: Supply of pickup p 1 /…**

**Publication reference:** **088-Supply- 02**

**Columns 1-2 should be completed by the contracting authority**

**Columns 3-4 should be completed by the tenderer**

**Column 5 is reserved for the evaluation committee**

Annex III - the contractor's technical offer

The tenderers are requested to complete the template on the next pages:

* Column 2 is completed by the contracting authority shows the required specifications (not to be modified by the tenderer),
* Column 3 is to be filled in by the tenderer and must detail what is offered (for example the words ‘compliant’ or ‘yes’ are not sufficient)
* Column 4 allows the tenderer to make comments on its proposed supply and to make eventual references to the documentation

The eventual documentation supplied should clearly indicate (highlight, mark) the models offered and the options included, if any, so that the evaluators can see the exact configuration. Offers that do not permit to identify precisely the models and the specifications may be rejected by the evaluation committee.

The offer must be clear enough to allow the evaluators to make an easy comparison between the requested specifications and the offeredspecifications.

| **1.**  **Item number** | **2.**  **Specifications required** | **3.**  **Specifications offered** | **4.**  **Notes, remarks,  ref to documentation** | **5.**  **Evaluation committee’s notes** |
| --- | --- | --- | --- | --- |
| **1** | **High-speed pickup truck:**  -Coupe: double-cab pickup type and separate load space  -Length: minimum 5000 mm  -Wheelbase: minimum 3000 mm  -Number of places: 4+1  -Number of doors: 4  -Ground clearance: not less than 190 mm  -Useful load: minimum 950 kg.  -Engine: Diesel  -Working volume: minimum 1900 cm3, but not more than 2000 cm3.  -Maximum power: minimum 130 hp, but not more than 140 hp  -Combined fuel consumption: max.9,01/100 km.  -Gearbox: mechanical with manual gearshift  -Drive: 4x4-front and rear wheel drive, fast and slow speeds.  Equipment:  -Minimum 2pcs. Airbags  -ABS –anti- lock braking system  -Immobilizer  -Central locking with remote control  -Air conditioning  -Minimum 2 pcs. Electric windows  -El. Adjustable side mirrors  -A factory-built-in audio system  -Rims: at least 16 inches  Warranty: A minimum of 4 years or 100,00 km of mileage. |  |  |  |